   Windows 95, OSR2

   Introduction:
   -------------
   This document describes the procedure to install  Windows 95 and OSR2
   driver for D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \WIN95\DLKRTS.SYS

   Installing driver procedure on Microsoft Windows 95 :
   -----------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Windows 95, it will auto-detect your system configuration
      and find the adapter hardware.  ( If Win95 does not  prompt that it
      detects the PCI Ethernet adapter, there must be something wrong with
      the D-Link DFE-530TX+ PCI Adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select 
         "Driver from disk provided by hardware manufacturer".

      2. Insert the DFE-530TX+ driver disk into CD-ROM drive and 
         specify the setup file pathname ,EX: E:\WIN95.

      3. Windows 95 will appear some messages to insert Windows 95 system
         disk to complete setup step.

      4. Windows 95 will finish the other installation procedure
         automatically, then you restart the system.
         