   LAN Server 2.0/3.0

   Introduction:
   -------------
   This document describes the procedure to install NDIS driver on DOS
   LAN Requester for D-Link DFE-530TX+ 
   PCI Adapter.

   Location of Driver:  \NDIS2\DOS\DLKRTS.DOS  (for DOS LAN Requester)
                        
   Installing driver procedure on DOS LAN Requester :
   --------------------------------------------------

      1. Insert the IBM LAN Support Program (LSP) Version 1.30 (or 1.31)
         Disk into your CD-ROM drive:

      2. EX:
         Type E:\dxmaid  and press <Enter> .

      3. The screen will display the IBM logo. Press <Enter> twice until
         the "Environment Information" appears on screen.

      4. Responds to the screen prompts, specifying the following values
         for each field,use the <Space Bar> to toggle between choices:

                Configuration for this computer?          Yes
                Use existing configuration information?   Yes
                Do you have adapter option diskettes?     Yes
                Are you configuring for two adapters?     No
                Do you need 802.2 interface support?      Yes
                
                EX:
                Source for LSP                           E:\
                
                Target for new configuration             C:\LSP

         Make sure that the values given above are correct, then press
         <Enter> to store your choices.

      5. Insert the D-Link DFE-530TX+ driver disk into CD-ROM drive,and 
         specify your pathname , EX: E:\NDIS2\DOS, then press ENTER.

      6. Follow  screen  instructions  to  complete  the  process. Simply
         pressing <Enter> for each screen display will select the default
         options. Press <Enter> until you reach the display prompting you
         to insert the LSP disk.

      7. Insert the LSP disk as prompted. Press <Enter> to acknowledge
         completion of the action.

      8. A screen  showing  the  current  configuration  detected will be
         displayed. It should show "D-Link DFE-530TX+ PCI Adapter"
         and the protocols already selected (i.e., "IBM IEEE 802.2" and
         "IBM OS/2 NETBIOS").

      9.  Press <F4>. to save the new configuration. This completes the 
          LSP installation.

      10. Save the configuration and reboot your computer.

      11. Insert the DOS LAN Requester Install Diskette 1 into your floppy
          drive.

      12. Type A:\INSTALL    <Enter>

      13. The IBM logo will again appear on the screen. Press <Enter> to
          move on to the next screen.

      14. Follow  screen  instructions,  pressing  <Enter>  to move from
          screen-to-screen until you are prompted to indicate the pathname
          of the DOS LAN Requester directory (C:\DOSLAN ).

      15. Specify the pathname (C:\DOSLAN is the default) for the DOS LAN
          Requester directory . Then press <Enter> to continue.

      16. The program will ask you for the services that you require.

      17. Highlight the appropriate option. Select either "Send messages"
          or "Send, View, Edit, and Log message" option. (Normally, second
          option "Send, View, Edit and Log message" is selected).

      18. Specify the PC's ID and domain ID.

      19. Follow screen prompts to complete the installation.

   Note:
   -----
   1. The DOS version must be bellow DOS 5.0 when install DOS LAN requester
      into your system.

   2.sample protocol.ini:


         [DLKRTL]
         DriverName=DLKRTS$
         EtherID=@52544C111111  ;This keyword is used to desinate a DFE-530TX+
                                ;adapter by assigning it's ethernet ID
                                ;when more than one adapters exist on one
                                ; system.

         Medium= _Auto, _10Half, _10Full, _100half, _100Full      
                            ;This keyword is used to force DFE-530TX+ adapter
                            ;to speed 10M or 100M mode. If not present,
                            ;the driver will auto-detect the speed.
                            