   LANtastic 6.0

   Introduction:
   -------------
   This document describes the procedure to setup NDIS driver on
   LANtastic 6.0 operation system for D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \NDIS2\DOS\DLKRTS.DOS

   Sample Configuration Files:
   --------------------------
     CONFIG.SYS:
         DEVICE=C:\LANTASTI\PROTMAN.DOS /I:C:\LANTASTI
         DEVICE=C:\LANTASTI\DLKRTS.DOS
         FILES=40
         BUFFERS=30

     STARTNET.BAT:
         @echo off
         rem LANtastic  Version 6.00  installed 95/05/23 14:11:21
         rem (for Windows)
         C:
         cd C:\LANTASTI
         SET LAN_CFG=C:\LANTASTI
         rem If LANtastic is disabled, skip everything.
         IF EXIST DISABLED GOTO :STARTNET_DONE
         @echo ===== Begin LANtastic configuration =====
         PATH C:\LANTASTI;C:\LANTASTI\NW;%PATH%
         SET LAN_DIR=C:\LANTASTI.NET
         SET NWDBPATH=C:\LANTASTI\NW
         rem Please obtain the NETBEUI.EXE program from Microsoft
         rem LOADHIGH NETBEUI
         LOADHIGH AI-NDIS BIND_TO=DLKRTS_NIF
         AILANBIO @STARTNET.CFG
         REDIR TEST @STARTNET.CFG
         IF EXIST NOSHARE GOTO :NOSHARE
         SERVER C:\LANTASTI.NET @STARTNET.CFG
         NET LOGIN \\TEST
         GOTO :CONTINUE
         :NOSHARE
         @echo LANtastic server was installed but turned off.
         :CONTINUE
         rem If CONNECT.BAT exists, run it to set up connections.
         IF EXIST CONNECT.BAT GOTO :CONNECT
         rem Otherwise set up connections specified during install.
         NET LPT TIMEOUT 10
         GOTO :CONNECT_DONE
         :CONNECT
         @echo Setting up LANtastic connections from CONNECT.BAT
         rem Build CONNECT.BAT like this: "NET SHOW/BATCH >
         C:\LANTASTI\CONNECT.BAT"
         rem   (or run the batch file SETNET.BAT)
         call CONNECT.BAT
         :CONNECT_DONE
         NET POSTBOX
         @echo ===== End LANtastic configuration =====
         :STARTNET_DONE
         cd \


         PROTOCOL.INI:

         ;PROTOCOL.INI for LANtastic Version 6.00
         ;------------ using
         ;
         [PROTMAN]
           DRIVERNAME = PROTMAN$
           DYNAMIC = YES

         [DLKRTS_NIF]
             DRIVERNAME = DLKRTS$
             Adapters=DFE-530TX+
            ;EtherID =@0123456789AB


   Install D-Link drivers for LANtastic 6.0 : (Using NDIS driver)
   ------------------------------------------
      The  installation  procedure  will  transfer  files  to a  specific
      directory on the workstation and modify existing configuration files
      to fit your specific needs.  The installation utility INSTALL.EXE is
      located on LANtastic Network Software Disk 1.   Run INSTALL.EXE from
      Disk 1  and  the  LANtastic  Install program screen will appear. You
      must  complete each of the questions.  These options are specific to
      your needs.

      1. Prompt you to enter a unique Computer Name.

      2. Ask you to select the drive that you want LANtastic to
         be installed on. The default is Drive C:.

      3. Ask you to specify a directory where you want the
         LANtastic files to be installed. The default is \LANTASTI.

      4. Ask you if you want to Share your Computers Drives or Printers.

      5. Ask you to select the Maximum Number of Connected Computers.

      6. Prompt you to select any other LANtastic features that you may 
         want to install.

      7. A summary screen of the options you will appear. If it
         looks correct continue with the installation.

      8. Prompt you to select a network adapter to run your
         LANtastic software on. From the list of adapters , select
         "NDIS SUPPORT FOR NETWORK ADAPTERS".

      9. Ask you to insert the manufacturers  driver disk containing the 
         driver files. Insert the DFE-530TX+ driver disk into CD-ROM drive
         and specify the source path for driver files, EX: E:\

     10. Ask you if you want to Set Up Permanent Drive or Printer
         Connections.

     11. Another summary screen of the options will appear. If
         this looks correct then select Perform the Installation
         and LANtastic will now install the files.
         