   Packet Driver

   Introduction:
   -------------
   This document describes the procedure to setup the Packet driver for
   D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \PKTDRV\DLKPKT.COM

   Sample Configuration Files:
   ---------------------------
      AUTOEXEC.BAT
      DLKPKT 0x60

   Notes:
   ------
     1. Load the packet driver using the software interrupt and any
        optional switches if required.

        Usage: DLKPKT [options] <software_int_no> [media type]

        Example: DLKPKT -i 0x7e

        The only required  parameter is the software interrupt. A packet
        driver needs to have a software interrupt assigned to it for other
        programs to access it. The recommended interrupt 0x7e. If you need
        any of the options listed below, place them before the software
        interrupt on the command line.

        -i - Force driver to report itself as 802.3 instead of Ethernet II.
        -d - Delayed initialization. Used for diskless booting
        -n - NetWare conversion. Converts 802.3 packets into 8137 packets
        -w - Windows hack, obsoleted by winpkt
        -p - Promiscuous mode disable
        -h - Help
        -u - Uninstall

     2. Media type can be used to force the card to work on specific
        speed and duplex mode. If no media type if specified, then
        driver will read hardware configuration from EEPROM on the
        card. The hardware configuration can be modified by running
        'DIAG' on driver disk.

     3. Type command,C:\DLKPKT 0x60, the screen will appear following
        message:

        System: [345]86 processor, PCI bus, Two 8259s
        Packet driver software interrupt is 0x60
        Interrupt number is 0x9
        I/O port is 0x6100
        My Ethernet address is 00:80:C8:29:29:AD

     4. Installing Multiple LAN Adapters:

        If there are multiple network cards on the main board. the user
        run DLKPKT 0x60 directly, then the screen will display :

        Packet driver for DFE-530TX+, PCI version 1.00
        Copyright 1997 (c), D-Link Corporation.

        There are 2 network cards on your main board :
        Card 1. IRQ= 0x9  I/O= 0x6100  NodeID= 00:80:C8:29:29:AD
        Card 2. IRQ= 0xA  I/O= 0x6000  NodeID= 00:80:C8:29:29:64
        Please select a Card No.(1-2): 1

        System: [345]86 processor, PCI bus, Two 8259s
        Packet driver software interrupt is 0x60
        Interrupt number is 0x9
        I/O port is 0x6100
        My Ethernet address is 00:80:C8:29:29:AD

     5. Installing multiple drivers:

        If you want to install multiple cards each connecting to different
        network, you have to install the driver multiple times, each with
        different packet interrupt number. Then modify 'ioaddr' variable
        in 'config.tel' to specify the packet inetrrupt you will use.
        