   Windows 98

   Introduction:
   -------------
   This document describes the procedure to install  Windows 98 driver 
   for D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \WIN98\DLKRTS.SYS

   Installing driver procedure on Microsoft Windows 98 :
   -----------------------------------------------------
      Before you start with the installation process, make sure that your
      adapter should be properly installed in your PCI bus slot.
      Executing Windows 98, it will auto-detect your system configuration
      and find the adapter hardware. ( If Win98 does not  prompt that it
      detects the PCI Ethernet adapter,there must be something wrong with
      the DFE-530TX+ PCI Fast Ethernet adapter or your system enviroment.)

      1. Ask you to select which driver you want to install, select 
         "Search for the best driver for your device".

      2. Insert the DFE-530TX+ driver disk into CD-ROM driver,
         select "specify a location" and specify the setup file pathname 
         ,EX: E:\WIN98.

      3. Windows 98 will appear some messages to insert Windows 98 system
         disk to complete setup step.

      4. Windows 98 will finish the other installation procedure 
         automatically then you restart the system.
         