   Server Driver for NetWare 3.12

   Introduction:
   -------------
   This document describes the procedure to install the NetWare v3.12
   server driver for D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \NWSERVER\312\DLKRTS.LAN


   Installation Procedure:
   -----------------------
      Before you start with the installation process, make sure that
      the Novell NetWare v3.12 server is properly installed.
      Similarly, your adapter should also be properly installed in your
      server.

      1. These files can be obtained from driver disk subdirectory
         \NWSERVER\312

         NBI31X.NLM
         MSM31X.NLM
         ETHERTSM.NLM

      2. If you can log into the server as a supervisor , copy DLKRTS.LAN
         relative files from the Driver Disk subdirectory, EX:
         E:\NWSERVER\312 into the NetWare 386 subdirectory SYSTEM of your
         server. (If some files exists, rename the existing files in the
         SYSTEM subdirectory).

      3. When the NetWare server prompt appears (indicated by a colon),
         load your server driver. Simply type:

         : LOAD NBI31X <Entet>
         : LOAD DLKRTS <Enter>

         or,
         you can directly load file from DFE-530TX+ driver disk :

         : LOAD A:\NWSERVER\312\NBI31X <Enter>
         : LOAD A:\NWSERVER\312\DLKRTS <Enter>

      4. Bind IPX to the adapter driver. At the NetWare server prompt
         ,type:

         :BIND IPX TO DLKRTS <Enter>

      5. After pressing <Enter> the computer prompts you for the Network
         Number. For details on how to assign this number,please consult
         your NetWare Server Installation Manual.

      6. Add the load and bind statements you require to the server's
         AUTOEXEC.NCF file so that the LAN driver will load automatically
         each time the server starts up.


   NOTES:
   ------
   1.Installing Multiple LAN Adapters:
     The keyword "SLOT" is provided for multiple LAN adapters in a
     single server by the driver RTSSRV.LAN. So, add EtherID in LOAD
     commands. For example:

     LOAD DLKRTS SLOT=1 FRAME=Ethernet_802.2 NAME=LAN_A 
     BIND IPX TO LAN_A NET=11
     LOAD DLKRTS SLOT=2 FRAME=Ethernet_802.2 NAME=LAN_B 
     BIND IPX TO LAN_B NET=22

   2. The keyword "MEDIUMTYPE" is provided for specifying adapter's 
      speed (AUTO, 100FULL, 100HALF, 10FULL, 10HALF), add SPEED in 
      LOAD commands. 
      For example:

      LOAD DLKRTS SLOT=1 MEDIUMTYPE=100HALF FRAME=Ethernet_802.2 NAME=LAN_A 
      BIND IPX TO LAN_A NET=11

   3. Installing One LAN adapter with Multiple Frame Types:
      When binding multiple frame types to one adapter, enter a LOAD
      and BIND statement for each frame type. Each LOAD statement will
      use a different network number is required on the bind statement.
      You need to supply a name on each load line in order to avoid
      being  prompted  for which  board to bind IPX to. If you do not
      have the name option in the AUTOEXEC.NCF , it will not  execute
      completely without user intervention. Example:

        LOAD DLKRTS FRAME=ETHERNET_802.3 NAME=IEE8023
        BIND IPX TO IEE8023 NET=11111
        LOAD DLKRTS FRAME=ETHERNET_802.2 NAME=IEE8022
        BIND IPX TO LAN8022 NET=22222

   If problems occur during the binding process, your screen will prompt
   you with error messages. Please refer to your NetWare 386 manual for
   details on these messages.
   