   Netware Client32 Driver for DOS/Windows 3.1x

   Introduction:
   -------------
   This document describes the procedure to install the NetWare Client32
   driver for D-Link DFE-530TX+ PCI Adapter.

   Location of Driver:     \NWCLIENT\CLIENT32\DLKRTS.LAN


   Sample Configuration Files:
   ---------------------------
      STARTNET.BAT (Client 32 for DOS will contain):

          C:\NOVELL\CLIENT32\NIOS.EXE
          LOAD C:\NOVELL\CLIENT32\LSLC32.NLM
          LOAD C:\NOVELL\CLIENT32\CMSM.NLM
          LOAD C:\NOVELL\CLIENT32\ETHERTSM.NLM
          LOAD C:\NOVELL\CLIENT32\DLKRTS.LAN FRAME=ETHERNET_802.2
          LOAD C:\NOVELL\CLIENT32\DLKRTS.LAN FRAME=Ethernet_802.3
          LOAD C:\NOVELL\CLIENT32\DLKRTS.LAN FRAME=Ethernet_II
          LOAD C:\NOVELL\CLIENT32\DLKRTS.LAN FRAME=Ethernet_SNAP

   A. Driver Installation Procedures on Clien32 for DOS :
   ------------------------------------------------------
     1.If you have completed installed the Netware Client 32 for DOS, all
       you have to do is to modify STARTNET.BAT.  Please see the sample
       STARTNET.BAT above. If not, Please follow the next step 2 - step 7.

     2.Run INSTALL.EXE from Netware Client 32 for DOS diskette 1 (or from
       Netware 4.11 CD).  When  the  product  manual  appears,  mark the
       "Netware Client 32 for DOS" item, then press <Enter>.

     3.Select "OTHER DRIVERS" item from "32-bit Network Board Drivers" 
       menu, then press <Enter>.

     4.Insert DFE-530TX+ Driver Disk, then specify the path 
       that matches the CD-ROM drive on your system.

     5.Select "D-Link DFE-530TX+ PCI Adapter Driver" then press <Enter>.

     6.Following instructions to complete the Client32 for DOS software
       installation.

     7.Reboot your machine.

      Installation Notes:
      -------------------
      * Installing Multiple LAN Adapters:
         The keyword  "SLOT"  is provided for multiple  LAN  adapters in a
         single server by the driver DLKRTS.LAN. So, add "SLOT"  in LOAD
         commands. For example:

         C:\NOVELL\CLIENT32\NIOS.EXE
         LOAD LSLC32.NLM
         LOAD CMSM.NLM
         LOAD ETHERTSM.NLM
         LOAD DLKRTS FRAME=Ethernet_802.2 SLOT=1
         LOAD DLKRTS FRAME=Ethernet_802.2 SLOT=2

   B. Driver Installation Procedures on Client32 for Windows 3.x :
   ---------------------------------------------------------------
     Refer to Content A. On step 2, mark "Netware Client 32 for DOS"  and
     "Client 32 for Windows". On step 4, specify  the path that matches 
     the CD-ROM drive on your system. Like
     E:\NWCLIENT\CLIENT32\DLKRTS.LAN , then  following step  3..7  to
     complete the installation.
     