

;******************************************************************************
;**                                                                          **
;**  Copyright 2007-2012 Intel Corporation All Rights Reserved.              **
;**                                                                          **
;**  The material contained or described herein and all documents related    **
;**  to such material ("Material") is owned by Intel Corporation or its      **
;**  suppliers or licensors, and title to such Material remains with Intel   **
;**  Corporation or its suppliers or licensors. The Material contains        **
;**  proprietary information of Intel or its suppliers and licensors. The    **
;**  Material is protected by worldwide copyright laws and treaty            **
;**  provisions. No part of the Material may be used, copied, reproduced,    **
;**  modified, published, uploaded, posted, transmitted, distributed or      **
;**  disclosed in any way without Intel's prior express written permission.  **
;**  No license under any patent, copyright or other intellectual property   **
;**  rights in the Material is granted to or conferred upon you, either      **
;**  expressly, by implication, inducement, estoppel or otherwise. Any       **
;**  license under such intellectual property rights must be express and     **
;**  approved by Intel in writing.                                           **
;**                                                                          **
;**  Unless otherwise agreed by Intel in writing, you may not remove or      **
;**  alter this notice or any other notice embedded in Materials by Intel    **
;**  or Intel’s suppliers or licensors in any way.                           **
;******************************************************************************
;
;******************************************************************************

; e1rxp5132.INF (Windows XP based 32 bit and
; Windows Server 2003 based 32 bit OSes)

;
; Intel(R) Gigabit Adapters
;******************************************************************************
;

[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Intel%
CatalogFile = e1rxp5132.cat
DriverVer   = 10/19/2012,12.3.35.0

[Manufacturer]
%Intel%     = Intel, NTx86.5.1, NTIA64, NTAMD64, NTx86.6.0

[ControlFlags]
ExcludeFromSelect = *

[Intel]

[Intel.NTx86.5.1]
; DisplayName                   Section                DeviceID
; -----------                   -------                --------
%E1533NC.DeviceDesc%            = E1533,               PCI\VEN_8086&DEV_1533
%E1536NC.DeviceDesc%            = E1536,               PCI\VEN_8086&DEV_1536
%E1537NC.DeviceDesc%            = E1536,               PCI\VEN_8086&DEV_1537
%E1538NC.DeviceDesc%            = E1538,               PCI\VEN_8086&DEV_1538
%E1539NC.DeviceDesc%            = E1539,               PCI\VEN_8086&DEV_1539
%E1533NCT1.DeviceDesc%          = E1533,               PCI\VEN_8086&DEV_1533&SUBSYS_00018086
%E1533NCT1.DeviceDesc%          = E1533,               PCI\VEN_8086&DEV_1533&SUBSYS_00028086
%E1533NCT1.DeviceDesc%          = E1533,               PCI\VEN_8086&DEV_1533&SUBSYS_0003103C

[Intel.NTIA64]

[Intel.NTamd64]

[Intel.NTx86.6.0]
;===============================================================================
;

;                     WINDOWS XP / Server 2003 PLATFORMS

;
;===============================================================================

;-------------------------------------------------------------------------------
; Intel(R) I210 Gigabit Network Connection
;-------------------------------------------------------------------------------
[E1533]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1r.reg, tso.reg, ResetLink.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Copper.reg, Copper1000.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = DCA.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS4Q.reg
AddReg             = Client.reg
AddReg             = EEE.reg
AddReg             = ReduceSpeedOnPowerDown.reg
AddReg             = Uninstall.reg, Uninstall.reg.winxp
CopyFiles          = winxp.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1533.Services]
AddService = e1rexpress, 2, winxp.Service, winxp.EventLog

[E1533.CoInstallers]
AddReg             = CoInstaller_AddReg, CoInKS.reg
CopyFiles          = CoInstaller_CopyFiles

[E1533.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired

;-------------------------------------------------------------------------------
; Intel(R) I211 Gigabit Network Connection
;-------------------------------------------------------------------------------
[E1539]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1r.reg, tso.reg, ResetLink.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Copper.reg, Copper1000.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = DCA.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS4Q.reg
AddReg             = Client.reg
AddReg             = EEE.reg
AddReg             = ReduceSpeedOnPowerDown.reg
AddReg             = Uninstall.reg, Uninstall.reg.winxp
CopyFiles          = winxp.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1539.Services]
AddService = e1rexpress, 2, winxp.Service, winxp.EventLog

[E1539.CoInstallers]
AddReg             = CoInstaller_AddReg, CoInKS.reg
CopyFiles          = CoInstaller_CopyFiles

[E1539.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired

;-------------------------------------------------------------------------------
; Intel(R) I210 Gigabit Fiber Network Connection
;-------------------------------------------------------------------------------
[E1536]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1r.reg, tso.reg, ResetLink.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = DCA.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS4Q.reg
AddReg             = Client.reg
AddReg             = Uninstall.reg, Uninstall.reg.winxp
CopyFiles          = winxp.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1536.Services]
AddService = e1rexpress, 2, winxp.Service, winxp.EventLog

[E1536.CoInstallers]
AddReg             = CoInstaller_AddReg, CoInKS.reg
CopyFiles          = CoInstaller_CopyFiles

[E1536.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired

;-------------------------------------------------------------------------------
; Intel(R) I210 Gigabit Network Connection
;-------------------------------------------------------------------------------
[E1538]
Characteristics    = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType            = 5    ; PCI
Port1FunctionNumber = 0
DelReg             = Advanced.DelReg
AddReg             = e1r.reg, tso.reg, ResetLink.reg, JumboPacket.reg
AddReg             = EnableWakeOnManagmentOnTCO.reg
AddReg             = Copper.reg, Copper1000.reg
AddReg             = Powermgmt.reg, WakeOnSlot.reg, WakeOnLink.reg
AddReg             = DCA.reg
AddReg             = LLI.reg
AddReg             = RSS.reg, RSS4Q.reg
AddReg             = Client.reg
AddReg             = Uninstall.reg, Uninstall.reg.winxp
CopyFiles          = winxp.CopyFiles, UninstallProg.CopyFiles
*IfType            = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType         = 0     ; NdisMedium802_3
*PhysicalMediaType = 14 ; NdisPhysicalMedium802_3

[E1538.Services]
AddService = e1rexpress, 2, winxp.Service, winxp.EventLog

[E1538.CoInstallers]
AddReg             = CoInstaller_AddReg, CoInKS.reg
CopyFiles          = CoInstaller_CopyFiles

[E1538.HW]
Include            = machine.inf
Needs              = PciIoSpaceNotRequired

;-------------------------------------------------------------------------------
; Do-nothing section used to avoid "Unknown hardware" installation prompts.
;
[NO_DRV]
Characteristics    = 0x01
Include            = machine.inf
Needs              = NO_DRV

[NO_DRV.Services]
Include            = machine.inf
Needs              = NO_DRV.Services

;-------------------------------------------------------------------------------
; Registry Settings (decimal)
;
[e1r.reg]
HKR, Ndi\Interfaces,                                    UpperRange,             0, "ndis5"
HKR, Ndi\Interfaces,                                    LowerRange,             0, "ethernet"
HKR, Ndi,                                               Service,                0, "e1rexpress"
HKR, Ndi\Params\*FlowControl,                           ParamDesc,              0, %FlowControl%
HKR, Ndi\Params\*FlowControl,                           default,                0, "3"
HKR, Ndi\Params\*FlowControl\Enum,                      "0",                    0, %Disabled%
HKR, Ndi\Params\*FlowControl\Enum,                      "1",                    0, %FlowControl_TxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "2",                    0, %FlowControl_RxOnly%
HKR, Ndi\Params\*FlowControl\Enum,                      "3",                    0, %FlowControl_Full%
HKR, Ndi\Params\*FlowControl,                           type,                   0, "enum"

; *TransmitBuffers
HKR, Ndi\params\*TransmitBuffers,                       ParamDesc,              0, %TransmitBuffers%
HKR, Ndi\params\*TransmitBuffers,                       default,                0, "512"
HKR, Ndi\params\*TransmitBuffers,                       min,                    0, "80"
HKR, Ndi\params\*TransmitBuffers,                       max,                    0, "2048"
HKR, Ndi\params\*TransmitBuffers,                       step,                   0, "8"
HKR, Ndi\params\*TransmitBuffers,                       Base,                   0, "10"
HKR, Ndi\params\*TransmitBuffers,                       type,                   0, "int"

; *ReceiveBuffers
HKR, Ndi\params\*ReceiveBuffers,                        ParamDesc,              0, %ReceiveBuffers%
HKR, Ndi\params\*ReceiveBuffers,                        default,                0, "256"
HKR, Ndi\params\*ReceiveBuffers,                        min,                    0, "80"
HKR, Ndi\params\*ReceiveBuffers,                        max,                    0, "2048"
HKR, Ndi\params\*ReceiveBuffers,                        step,                   0, "8"
HKR, Ndi\params\*ReceiveBuffers,                        Base,                   0, "10"
HKR, Ndi\params\*ReceiveBuffers,                        type,                   0, "int"

; *TCPChecksumOffloadIPv4
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                ParamDesc,              0, %TCPChksumOffv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,                type,                   0, "enum"

; *UDPChecksumOffloadIPv4
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                ParamDesc,              0, %UDPChksumOffv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                default,                0, "3"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "0",                    0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\Enum,           "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,                type,                   0, "enum"

; *IPChecksumOffloadIPv4
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 ParamDesc,              0, %IPChksumOffv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 default,                0, "3"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "0",                    0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "1",                    0, %ChksumOffTx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "2",                    0, %ChksumOffRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\Enum,            "3",                    0, %ChksumOffTxRx%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,                 type,                   0, "enum"

; Network Address
HKR, Ndi\params\NetworkAddress,                         ParamDesc,              0, %LAA%
HKR, Ndi\params\NetworkAddress,                         Default,                0, ""
HKR, Ndi\params\NetworkAddress,                         type,                   0, "edit"
HKR, NDI\params\NetworkAddress,                         LimitText,              0, "12"
HKR, NDI\params\NetworkAddress,                         UpperCase,              0, "1"
HKR, NDI\params\NetworkAddress,                         optional,               0, "1"

;Log Link State Event
HKR,Ndi\Params\LogLinkStateEvent,                       ParamDesc,              0, %LogLinkState%
HKR,Ndi\Params\LogLinkStateEvent,                       Type,                   0, "enum"
HKR,Ndi\Params\LogLinkStateEvent,                       Default,                0, "51"
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "51",                   0, %Enabled%
HKR,Ndi\Params\LogLinkStateEvent\Enum,                  "16",                   0, %Disabled%
HKR,,                                                   LogLinkStateEvent,      0, "51"

; Wait for Link
HKR, Ndi\Params\WaitAutoNegComplete,                    ParamDesc,              0, %WaitAutoNegComplete%
HKR, Ndi\Params\WaitAutoNegComplete,                    default,                0, "2"
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "0",                    0, %Off%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "1",                    0, %On%
HKR, Ndi\Params\WaitAutoNegComplete\Enum,               "2",                    0, %AutoDetect%
HKR, Ndi\Params\WaitAutoNegComplete,                    type,                   0, "enum"

;  Interrupt Throttle Rate
HKR, Ndi\Params\ITR,                                    ParamDesc,              0, %InterruptThrottleRate%
HKR, Ndi\Params\ITR,                                    default,                0, "65535"
HKR, Ndi\Params\ITR\Enum,                               "65535",                0, %Adaptive%
HKR, Ndi\Params\ITR\Enum,                               "3600",                 0, %Extreme%
HKR, Ndi\Params\ITR\Enum,                               "2000",                 0, %High%
HKR, Ndi\Params\ITR\Enum,                               "950",                  0, %Medium%
HKR, Ndi\Params\ITR\Enum,                               "400",                  0, %Low%
HKR, Ndi\Params\ITR\Enum,                               "200",                  0, %Minimal%
HKR, Ndi\Params\ITR\Enum,                               "0",                    0, %Off%
HKR, Ndi\Params\ITR,                                    type,                   0, "enum"
HKR,,                                                   ITR,                    0, "65535"

; *PriorityVLANTag
HKR, Ndi\Params\*PriorityVLANTag,                       ParamDesc,              0, %PriorityVLANTag%
HKR, Ndi\Params\*PriorityVLANTag,                       default,                0, "3"
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "0",                    0, %PriorityVlanDisabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "1",                    0, %PriorityEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "2",                    0, %VlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag\Enum,                  "3",                    0, %PriorityVlanEnabled%
HKR, Ndi\Params\*PriorityVLANTag,                       type,                   0, "enum"

; EnablePME
HKR,Ndi\Params\EnablePME,                               ParamDesc,              0, %Enable_PME%
HKR,Ndi\Params\EnablePME,                               Type,                   0, "enum"
HKR,Ndi\Params\EnablePME,                               Default,                0, "0"
HKR,Ndi\Params\EnablePME\Enum,                          "1",                    0, %Enabled%
HKR,Ndi\Params\EnablePME\Enum,                          "0",                    0, %Disabled%

; Hardwired defaults
HKR,,                                                   PciScanMethod,          0, "3"
HKR,,                                                   TxIntDelay,             0, "28"
HKR,,                                                   MulticastFilterType,    0, "0"
HKR,,                                                   VlanFiltering,          0, "0"

; Advanced Power Consumption Features

[tso.reg]
; TcpSegmentation
HKR, Ndi\Params\TcpSegmentation,                        ParamDesc,              0, %TcpSegmentation%
HKR, Ndi\Params\TcpSegmentation,                        default,                0, "1"
HKR, Ndi\Params\TcpSegmentation\Enum,                   "0",                    0, %Off%
HKR, Ndi\Params\TcpSegmentation\Enum,                   "1",                    0, %On%
HKR, Ndi\Params\TcpSegmentation,                        type,                   0, "enum"

[Copper.reg]
HKR, Ndi\params\*SpeedDuplex,                           ParamDesc,              0, %SpeedDuplex%
HKR, Ndi\params\*SpeedDuplex,                           default,                0, "0"
HKR, Ndi\params\*SpeedDuplex,                           type,                   0, "enum"
HKR, Ndi\params\*SpeedDuplex\enum,                      "0",                    0, %AutoNegotiation%
HKR, Ndi\params\*SpeedDuplex\enum,                      "1",                    0, %10Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "2",                    0, %10Mb_Full_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "3",                    0, %100Mb_Half_Duplex%
HKR, Ndi\params\*SpeedDuplex\enum,                      "4",                    0, %100Mb_Full_Duplex%
HKR, PROSetNdi\NdiExt\Params\*SpeedDuplex,              ExposeLevel,            0, "3"

; AutoNegAdvertised
HKR, PROSetNdi\Params\AutoNegAdvertised,                ParamDesc,              0, %AutoNegAdvertised%
HKR, PROSetNdi\Params\AutoNegAdvertised,                default,                0, "47"
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "1",                    0, %Advertise_10_Half%
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "2",                    0, %Advertise_10_Full%
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "4",                    0, %Advertise_100_Half%
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "8",                    0, %Advertise_100_Full%
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "47",                   0, %AutoNegAdvSpdDefault%
HKR, PROSetNdi\Params\AutoNegAdvertised,                type,                   0, "bitfield"
HKR, PROSetNdi\Params\AutoNegAdvertised,                ExposeLevel,            0, "3"
HKR,,                                                   AutoNegAdvertised,      2, "47"

[Copper1000.reg]
HKR, Ndi\params\*SpeedDuplex\enum,                      "6",                    0, %1000Mb_Full_Duplex%
HKR, PROSetNdi\Params\AutoNegAdvertised\Enum,           "32",                   0, %Advertise_1000_Full%

; Gigabit Master Slave Mode
HKR,Ndi\Params\MasterSlave,                             ParamDesc,              0, %MasterSlaveMode%
HKR,Ndi\Params\MasterSlave,                             Type,                   0, "enum"
HKR,Ndi\Params\MasterSlave,                             Default,                0, "0"
HKR,Ndi\Params\MasterSlave\Enum,                        "0",                    0, %AutoDetect%
HKR,Ndi\Params\MasterSlave\Enum,                        "1",                    0, %GigabitMasterMode%
HKR,Ndi\Params\MasterSlave\Enum,                        "2",                    0, %GigabitSlaveMode%

[ReduceSpeedOnPowerDown.reg]
; ReduceSpeedOnPowerDown
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  ParamDesc,              0, %ReduceSpeedOnPowerDown%
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  Type,                   0, "enum"
HKR,Ndi\Params\ReduceSpeedOnPowerDown,                  Default,                0, "1"
HKR,Ndi\Params\ReduceSpeedOnPowerDown\Enum,             "1",                    0, %Enabled%
HKR,Ndi\Params\ReduceSpeedOnPowerDown\Enum,             "0",                    0, %Disabled%
HKR,,                                                   ReduceSpeedOnPowerDown, 0, "1"

;-------------------------------------------------------------------------------
; Packet specifics
;

; *JumboPacket
[JumboPacket.reg]
HKR, Ndi\Params\*JumboPacket,                           ParamDesc,              0, %JumboPacket%
HKR, Ndi\Params\*JumboPacket,                           default,                0, "1514"
HKR, Ndi\Params\*JumboPacket\Enum,                      "1514",                 0, %Disabled%
HKR, Ndi\Params\*JumboPacket\Enum,                      "4088",                 0, %Bytes4088%
HKR, Ndi\Params\*JumboPacket\Enum,                      "9014",                 0, %Bytes9014%
HKR, Ndi\Params\*JumboPacket,                           type,                   0, "enum"

[Powermgmt.reg]
HKR, Ndi\Params\WakeOn,                                 ParamDesc,              0, %WakeOnSettings%
HKR, Ndi\Params\WakeOn\Enum,                            "0",                    0, %Disabled%
HKR, Ndi\Params\WakeOn\Enum,                            "2",                    0, %WakeOnMagicPacket%
HKR, Ndi\Params\WakeOn\Enum,                            "116",                  0, %WakeOnDirectedPacket%
HKR, Ndi\Params\WakeOn\Enum,                            "118",                  0, %WakeOnMagicAndDirectedPackets%
HKR, Ndi\Params\WakeOn\Enum,                            "246",                  0, %OSControlled%
HKR, Ndi\Params\WakeOn,                                 type,                   0, "enum"

[EEE.reg]
HKR, Ndi\Params\EEELinkAdvertisement,                   ParamDesc,              0, %EEELinkAdvertisement%
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "0",                    0, %EEE_Disabled%
HKR, Ndi\Params\EEELinkAdvertisement\Enum,              "1",                    0, %EEE_Enabled_AWAKE%
HKR, Ndi\Params\EEELinkAdvertisement,                   type,                   0, "enum"
HKR, Ndi\Params\EEELinkAdvertisement,                   default,                0, "1"

[WakeOnLink.reg]
HKR, Ndi\Params\WakeOnLink,                             ParamDesc,              0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,                        "0",                    0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,                        "2",                    0, %Forced%
HKR, Ndi\Params\WakeOnLink,                             type,                   0, "enum"
HKR, Ndi\Params\WakeOnLink,                             default,                0, "0"

[Client.reg]
HKR, Ndi\Params\WakeOn,                                 default,                0, "246"
HKR,,                                                   WakeOn,                 2, "246"

[ResetLink.reg]
HKR,,                                                   ResetLinkWA,            0, "1"

[RSS.reg]
; *RSS
HKR, Ndi\Params\*RSS,                                   ParamDesc,              0, %RSS%
HKR, Ndi\Params\*RSS,                                   default,                0, "1"
HKR, Ndi\Params\*RSS,                                   type,                   0, "enum"
HKR, Ndi\Params\*RSS\Enum,                              "0",                    0, %Disabled%
HKR, Ndi\Params\*RSS\Enum,                              "1",                    0, %Enabled%

[RSS2Q.reg]
; NumRssQueues
HKR, Ndi\Params\NumRssQueues,                           ParamDesc,              0, %NumRssQueues%
HKR, Ndi\Params\NumRssQueues,                           default,                0, "1"
HKR, Ndi\Params\NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\NumRssQueues\Enum,                      "2",                    0, %2queues%

[RSS4Q.reg]
; NumRssQueues
HKR, Ndi\Params\NumRssQueues,                           ParamDesc,              0, %NumRssQueues%
HKR, Ndi\Params\NumRssQueues,                           default,                0, "1"
HKR, Ndi\Params\NumRssQueues,                           type,                   0, "enum"
HKR, Ndi\Params\NumRssQueues\Enum,                      "1",                    0, %1queue%
HKR, Ndi\Params\NumRssQueues\Enum,                      "2",                    0, %2queues%
HKR, Ndi\Params\NumRssQueues\Enum,                      "4",                    0, %4queues%

[DCA.reg]
HKR, PROSetNdi\Params\EnableDca,                        ParamDesc,              0, %EnableDca%
HKR, PROSetNdi\Params\EnableDca,                        default,                0, "1"
HKR, PROSetNdi\Params\EnableDca,                        type,                   0, "enum"
HKR, PROSetNdi\Params\EnableDca\Enum,                   "1",                    0, %Enabled%
HKR, PROSetNdi\Params\EnableDca\Enum,                   "0",                    0, %Disabled%
HKR,,                                                   EnableDca,              2, "1"

[LLI.reg]
HKR, PROSetNdi\Params\EnableLLI,                        ParamDesc,              0, %EnableLLI%
HKR, PROSetNdi\Params\EnableLLI,                        default,                0, "0"
HKR, PROSetNdi\Params\EnableLLI,                        type,                   0, "enum"
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "0",                    0, %Disabled%
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "1",                    0, %LLIPortBased%
HKR, PROSetNdi\Params\EnableLLI\Enum,                   "2",                    0, %LLIPSHBased%
HKR,,                                                   EnableLLI,              2, "0"
HKR, PROSetNdi\Params\LLIPorts,                         ParamDesc,              0, %LLIPorts%
HKR, PROSetNdi\Params\LLIPorts,                         default,                0, ""
HKR, PROSetNdi\Params\LLIPorts,                         type,                   0, "edit"
HKR, PROSetNdi\Params\LLIPorts,                         UpperCase,              0, "1"
HKR, PROSetNdi\Params\LLIPorts,                         optional,               0, "1"
HKR, PROSetNdi\Params\LLIPorts,                         multi_string,           0, "1"
HKR,,                                                   LLIPorts,               0x00010002, ""

;-------------------------------------------------------------------------------
[WakeOnSlot.reg]
HKR,,                                                   WakeOnSlot,             0, 0

;-----------------------------------------------------------------------------
[WakeOnPort.reg]
HKR,,                                                   WakeOnPort,             0x00010001, 0

[EnableWakeOnManagmentOnTCO.reg]
HKR,,                                                   EnableWakeOnManagmentOnTCO, 0, "0"

;-------------------------------------------------------------------------------
; Uninstallation

[Uninstall.reg]
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1533, 0, "1533"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1536, 0, "1536"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1537, 0, "1537"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1538, 0, "1538"

[Uninstall.reg.winxp]
HKLM,Software\Intel\Prounstl\Dins, e1rxp5132.din, 0, "8254x.Uninstall"
HKLM,Software\Intel\Prounstl\Services, e1rexpress, 0, "e1rxp5132.sys"

[UninstallProg.CopyFiles]
e1rxp5132.din,,,2

;-------------------------------------------------------------------------------
; WinXP copy files
;

[winxp.CopyFiles]
e1rxp5132.sys,,,2

[winxp.Service]
DisplayName     = %E1RExpress.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e1rxp5132.sys
LoadOrderGroup  = NDIS

;-------------------------------------------------------------------------------
; Common base for all drivers for Eventlog and TextModeFlags
;

[winxp.EventLog]
AddReg             = winxp.AddEventLog.reg

[winxp.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %EventLogMessageDllPath%
HKR, , TypesSupported,   0x00010001, 7

;-------------- Coinstaller installation
[CoInstaller_CopyFiles]
NicCo2.dll,,,           0x00000010 ;don't overwrite
NicInE1R.dll
e1rmsg.dll

[CoInstaller_AddReg]
HKR,, CoInstallers32,   0x00010000, "NicCo2.dll,NicCoInstallerEntry"
HKR,, NicCoPlugins,     0x00010000, "NicInE1R.dll,NicCoInstallerEntry"

[CoInKS.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x80201001

[CoInKSQuadLOM.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x80201041

[CoInKMPQuadNIC.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x80201441

[CoInKMPWDualNIC.reg]
HKR,,                                          CoInstallFlag,      0x00010001, 0x80201441

;-------------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
DefaultDestDir                = 11
winxp.CopyFiles          = 12
UninstallProg.CopyFiles          = 11
CoInstaller_CopyFiles          = 11

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
e1rxp5132.din = 1
e1rxp5132.sys = 1
e1rmsg.dll = 1
NicCo2.dll = 1
NicInE1R.dll = 1

;-------------------------------------------------------------------------------
; Legacy
[Advanced.DelReg]
HKR, Ndi\Params
HKR, PROSetNdi\Params
HKR, PROSetNdi\NdiExt
HKR,, LinkNegotiationProcess

;-----------------------------------------------------------------------------
; Localizable Strings

[Strings]
AutoDetect                      = "Auto Detect"
AutoNegotiation                 = "Auto Negotiation"
Advertise_10_Half               = "Advertise 10 Half"
Advertise_10_Full               = "Advertise 10 Full"
Advertise_100_Half              = "Advertise 100 Half"
Advertise_100_Full              = "Advertise 100 Full"
Advertise_1000_Full             = "Advertise 1000 Full"
AutoNegAdvSpdDefault            = "Advertise Speed Default"
AutoNegAdvertised               = "Negotiable Speeds and Duplexes"
SpeedDuplex                     = "Speed & Duplex"
10Mb_Half_Duplex                = "10 Mbps Half Duplex"
10Mb_Full_Duplex                = "10 Mbps Full Duplex"
100Mb_Half_Duplex               = "100 Mbps Half Duplex"
100Mb_Full_Duplex               = "100 Mbps Full Duplex"
1000Mb_Full_Duplex              = "1.0 Gbps Full Duplex"
IPChksumOffv4                   = "IPv4 Checksum Offload"
TCPChksumOffv4                  = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4                  = "UDP Checksum Offload (IPv4)"
ChksumOffTxRx                   = "Rx & Tx Enabled"
ChksumOffTx                     = "Tx Enabled"
ChksumOffRx                     = "Rx Enabled"
TcpSegmentation                 = "Offload TCP Segmentation"
FlowControl                     = "Flow Control"
FlowControl_TxOnly              = "Tx Enabled"
FlowControl_RxOnly              = "Rx Enabled"
FlowControl_Full                = "Rx & Tx Enabled"
PriorityVlanDisabled            = "Priority & VLAN Disabled"
PriorityEnabled                 = "Priority Enabled"
VlanEnabled                     = "VLAN Enabled"
PriorityVlanEnabled             = "Priority & VLAN Enabled"
TransmitBuffers                 = "Transmit Buffers"
ReceiveBuffers                  = "Receive Buffers"
PriorityVLANTag                 = "Priority & VLAN"
RSS                             = "Receive Side Scaling"
NumRssQueues                    = "Receive Side Scaling Queues"
1queue                          = "1 Queue"
2queues                         = "2 Queues"
4queues                         = "4 Queues"
On                              = "On"
Off                             = "Off"
Enabled                         = "Enabled"
Disabled                        = "Disabled"
Bytes4088                       = "4088 Bytes"
Bytes9014                       = "9014 Bytes"
LAA                             = "Locally Administered Address"
JumboPacket                     = "Jumbo Packet"
WakeOnMagicPacket               = "Wake on Magic Packet"
Enable_PME                      = "Enable PME"
WakeOnSettings                  = "Wake on Settings"
WakeOnDirectedPacket            = "Wake on Directed Packet"
WakeOnMagicAndDirectedPackets   = "Wake on Magic & Directed"
OSControlled                    = "OS Controlled"
Forced                          = "Forced"
WakeOnLinkSettings              = "Wake on Link Settings"
LogLinkState                    = "Log Link State Event"
InterruptThrottleRate           = "Interrupt Moderation Rate"
Adaptive                        = "Adaptive"
Extreme                         = "Extreme"
Minimal                         = "Minimal"
High                            = "High"
Medium                          = "Medium"
Low                             = "Low"
GigabitMasterMode               = "Force Master Mode"
GigabitSlaveMode                = "Force Slave Mode"
MasterSlaveMode                 = "Gigabit Master Slave Mode"
WaitAutoNegComplete             = "Wait for Link"
EnableDca                       = "Direct Cache Access"
EnableLLI                       = "Low Latency Interrupts"
LLIPorts                        = "Low Latency Interrupt Ports"
LLIPortBased                    = "Port-Based"
LLIPSHBased                     = "PSH Flag-Based"
EEELinkAdvertisement            = "Energy Efficient Ethernet"
EEE_Disabled                    = "Off"
EEE_Enabled_AWAKE               = "On if system is awake"
ReduceSpeedOnPowerDown          = "Reduce Speed On Power Down"
Intel                           = "Intel"
EventLogMessageDllPath          = "%SystemRoot%\System32\netevent.dll;%SystemRoot%\System32\drivers\e1rxp5132.sys"
E1RExpress.Service.DispName     = "Intel(R) PCI Express Network Connection Driver R"
DISKNAME                        = "Intel(R) Driver Disk"

;; Brandnames.str
;------------------------------------------------------------------------------
E1533NC.DeviceDesc              = "Intel(R) I210 Gigabit Network Connection"
E1539NC.DeviceDesc              = "Intel(R) I211 Gigabit Network Connection"
E1536NC.DeviceDesc              = "Intel(R) I210 Gigabit Fiber Network Connection"
E1537NC.DeviceDesc              = "Intel(R) I210 Gigabit Backplane Connection"
E1538NC.DeviceDesc              = "Intel(R) I210 Gigabit Network Connection"
E1533NCT1.DeviceDesc            = "Intel(R) Ethernet Server Adapter I210-T1"

;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------
;---------------------------------------------------------------------------------------------------

